DATEX SMART TOUCH M: Control and supervision of dyeing machine. Machine visualization with manual function. Program editor & machine editor

Specification

* Display: 12” TFT color Touchscreen
* External I/O: Datex PLC Master
* Datex PLC module Digital & Analog – I/O
* Interface: 1 Ethernet, 2 USB
* Power Supply: 24v DC, 2.5 A
* Dimension: 319 x 226 x 90 mm( w x h x d)

## DATEX PLC MASTER 841616

**DATEX PLC SYSTEM** is an industry PLC with open source software, fully compatible with **DATEX**controller and Arduino. Open PLC project consist of two parts in our system: Runtime and Editor. HMI ScadaBR.

* Interface: Modbus RTU (USB)
* Display for Status IN/OUT
* Power: 24V DC
* Dimensions: 212 x 110 mm
* 16 Digital Outputs
* 14 Digital Inputs
* 2 Counter Inputs
* 4 Analog Outputs
* 2 PT100 Inputs  
  3-Wire
* 6 Analog Inputs