Landing:

1. MINIJET

Sample fabric dyeing

Range between: 1 to 5kg of fabric

Brand: UGOLINI – Italy

1. iPro

ATMOSPHERIC DYEING MACHINE

Brand:

1. iPro

HIGH TEMPERATURE DYEING MACHINE

Brand:

Description:

1. MINIJET

High temperature and high pressure fabric Sample dyeing machine

Suitable for dyeing in any type of fabrics natural or synthetic.

Liquor ratio of 1:5, Capacity range 1 to 5 kg

Brand: UGOLINI – Italy

More info(<https://www.ugolini.net/laboratory-apparatus-en-en-en/minijet-4/>)

1. iPro

ATMOSPHERIC DYEING MACHINE

Brand:

Range between 10 kgs to 2000 kgs

LIQUOR RATIO 1:3.7

FABRIC SPEED: 0-350M/MIN

WORKING TEMP.: MAX.98℃

Leveling Spray System, Crease preventive operation

Tangle free operation is a guarantee

Automatic Multi-level Adjustable Square/round Nozzle

Automatic Multi-level Chamber Adjustment System

Uniform Fabric Treatment even in open-width form

Water consumption – 25 to 40 liters / kg fabric, for light to dark shades.

1. iPro

HIGH TEMPERATURE DYEING MACHINE

Brand:

Range between 10 kgs to 2000 kgs

LIQUOR RATIO 1:3.7

FABRIC SPEED: 0-350M/MIN

WORKING TEMP.: MAX.98℃

Leveling Spray System, Crease preventive operation

Tangle free operation is a guarantee

Automatic Multi-level Adjustable Square/round Nozzle

Automatic Multi-level Chamber Adjustment System

Uniform Fabric Treatment even in open-width form

Water consumption – 25 to 40 liters / kg fabric, for light to dark shades.

Cotton, Modal, Viscose, Tencel, Rayon, Wool, Acrylic, Tencel, Lyocell, CVC, Nylon, Polyester blended and Lycra blended